Compaq Evo T20

In the end i gave up my efforts to make LTSP work on Evo T20… Probably it's not completely impossible, but its quite problematic and isn't worth the effort as it does not have gigabit NIC which is needed for LTSP to perform nicely…

Basic HOWTOs

http://wiki.wlug.org.nz/CompaqEvoT20Notes

http://mowson.org/karl/articles/t20-etherboot/

http://open-evot20.sourceforge.net/

PXE images

http://etherboot.org/

http://rom-o-matic.net/

Compile EtherBoot

Nastavíme

v Config

-DSIZEINDICATOR

-DASK_BOOT=1

v arch/i386/Config

-DCONFIG_PCI_DIRECT

Sestavíme

make ARCH=i386 bin/natsemi.zhd

Výsledný image je pak treba pomocí skriptu t20-etherboot.sh naflashovat do originálního image od výrobce.

Ten se liší podle konkrétního modelu (model number, případně konfigurace flash/ram)

Je potřeba ho rozbalit ze samorozbalovacího exe…

Configure LSTP

Kernel

kernel bez PAE - třeba i486 kernel z debianu

pnpbios=off