SDR Tools

GQRX - User friendly AM/FM/CW receiver GUI

GQRX scan - Script using GQRX for automatic scanning

Dump 1090 - ADS-B receiver with interactive map

RTL 433

Citizen weather sensors and remote controls in 433MHz ISM band

Should work with various sensors, eg.: http://www.tipa.eu/cz/cidlo-wh2wh1170/d-124298/

Supports 20+ devices

OOK Decoder

OOK decoder for 443MHz, 868MHz, etc…

Weather sensors, remote control

Only few sensors supported…

Tři Tchoři - efficient scanner (WIP)

SZDC - receive multiple channels at once

Find, fix and finish - simple weather sonde hunting and triangulation script

Tetra Listener - Multichannel RX/recorder for Tetra Network.